Special note for this work order:

1. **No new material is needed.** The student will drop-off the steel rod to be machined at the EDMC once their supervisor has approved the quotation.
2. Work description:
   1. Steel rod outer diameter reduced to 6.5mm for a length of 60mm from one end. (See drawing)
   2. Either end is fine.
3. If more dimensions are needed, or if the drawing is unclear, please contact the student at:
   1. [kwl1y19@soton.ac.uk](mailto:kwl1y19@soton.ac.uk) or
   2. +44 07778147127

Thank you!